EANCOM PART II |  | 1997-07-01

DEBMUL | - | Multiple debit advice message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 38 |  | Next Segment

SG4 | - | M | 9999 | - | LIN-DTM-BUS-MOA-SG5-SG6-SG7-SG10
SG10 | - | C | 9999 | - | SEQ-DTM-BUS-FII-SG11-SG12-SG13-SG14-SG15-SG16-SG17-SG20
SG16 | - | C | 10 | - | GIS-MOA-LOC-NAD-RCS-FTX
GIS | - | M | 1 | - | General indicator
Function:
To transmit a processing indicator.
EDIFACT
EAN
*
Description |
C529
PROCESSING INDICATOR
M |
M
| 7365
| Processing indicator, coded |
M |  | an..3
M
*
10 = Declaration requested
37 = Complete information
| 1131
| Code list qualifier |
C |  | an..3
N
| 3055
| Code list responsible agency, coded |
C |  | an..3
N
| 7187
| Process type identification |
C |  | an..17
N
Segment Notes:
This segment is used to indicate that the information contained in the following segments will be passed on to and processed by the central and regulatory party identified in the NAD segment. Note: The use of this segment group is subject to regulations stipulated by regulatory authorities, e.g. Central Bank. Example : GIS+10'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |