EANCOM PART II |  | 1997-07-01

HANMOV | - | Cargo/goods handling and movement message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 20 |  | Next Segment

SG7 | - | C | 99 | - | LIN-PIA-IMD-HAN-SG8-QTY-DTM-FTX-SG10-SG11
SG11 | - | C | 99 | - | PAC-MEA-QTY-SG12
PAC | - | M | 1 | - | Package
Function:
To describe the number and type of packages/physical units.
EDIFACT
EAN
*
Description |
7224
Number of packages
C |  | n..8
O
C531
PACKAGING DETAILS
C |
A
| 7075
| Packaging level, coded |
C |  | an..3
N
| 7233
| Packaging related information, coded |
C |  | an..3
O
50 = Package barcoded EAN-13 or EAN-8
51 = Package barcoded ITF-14 or ITF-6
52 = Package barcoded UCC or EAN-128
| 7073
| Packaging terms and conditions, coded |
C |  | an..3
O
1E = Unpack from (EAN Code)
2E = Repack in (EAN Code)
3E = Pack in (EAN Code)
C202
PACKAGE TYPE
C |
O
| 7065
| Type of packages identification |
C |  | an..17
A
PU = Tray
SL = Slipsheet
09 = Returnable pallet (EAN Code)
201 = Pallet ISO 1 - 1/1 EURO Pallet (EAN Code)
| 1131
| Code list qualifier |
C |  | an..3
O
| 3055
| Code list responsible agency, coded |
C |  | an..3
O
9 = EAN (International Article Numbering association)
| 7064
| Type of packages |
C |  | an..35
O
C402
PACKAGE TYPE IDENTIFICATION
C |
N
| 7077
| Item description type, coded |
M |  | an..3
| 7064
| Type of packages |
M |  | an..35
| 7143
| Item number type, coded |
C |  | an..3
| 7064
| Type of packages |
C |  | an..35
| 7143
| Item number type, coded |
C |  | an..3
C532
RETURNABLE PACKAGE DETAILS
C |
N
| 8395
| Returnable package freight payment responsibility, coded |
C |  | an..3
| 8393
| Returnable package load contents, coded |
C |  | an..3
Segment Notes:
This segment is used to specify the packaging details for the currently identified line item. When this segment is used for unpacking and re-packing purposes segment group 11 must be repeated to identify the 'unpack from' and 're-pack in' packages and any information associated with the unpack/re-pack, e.g. SSCC's. Example: PAC+10+:50+PK' This example details 10 packages barcoded with EAN-13 or EAN-8.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |