EANCOM PART II |  | 1997-07-01

HANMOV | - | Cargo/goods handling and movement message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 23 |  | Next Segment

SG7 | - | C | 99 | - | LIN-PIA-IMD-HAN-SG8-QTY-DTM-FTX-SG10-SG11
SG11 | - | C | 99 | - | PAC-MEA-QTY-SG12
SG12 | - | C | 9 | - | PCI-GIN
PCI | - | M | 1 | - | Package identification
Function:
To specify markings and labels on individual packages or physical units.
EDIFACT
EAN
*
Description |
4233
Marking instructions, coded
C |  | an..3
R
10 = Mark batch number
14 = Mark expiry date
16 = Buyer's instructions
17 = Supplier's instructions
18 = Carrier's instructions
30 = Mark serial shipping container code
31E = Mark price (EAN Code)
32E = Mark EAN/UPC number (EAN Code)
33E = Marked with serial shipping container code (EAN Code)
34E = Marked with EAN/UPC number (EAN Code)
C210
MARKS & LABELS
C |
O
| 7102
| Shipping marks |
M |  | an..35
M
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
8275
Container/package status, coded
C |  | an..3
O
C827
TYPE OF MARKING
C |
N
| 7511
| Type of marking, coded |
M |  | an..3
| 1131
| Code list qualifier |
C |  | an..3
| 3055
| Code list responsible agency, coded |
C |  | an..3
Segment Notes:
This segment is used to provide markings and labels information relevant to the packaging identified in the PAC segment. Example : PCI+30E' PCI+17+HANDLE WITH CARE'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |