EANCOM PART II |  | 1997-07-01

QALITY | - | Quality data message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 17 |  | Next Segment

SG5 | - | C | 200 | - | LIN-PIA-IMD-MEA-DTM-QTY-FTX-SG6-SG7-SG12
QTY | - | C | 99 | - | Quantity
Function:
To specify a pertinent quantity.
EDIFACT
EAN
*
Description |
C186
QUANTITY DETAILS
M |
M
| 6063
| Quantity qualifier |
M |  | an..3
M
*
74 = Latest cumulative quantity
79 = Previous cumulative quantity
99 = Estimated quantity
40E = Quantity tested (EAN Code)
| 6060
| Quantity |
M |  | n..15
M
| 6411
| Measure unit qualifier |
C |  | an..3
D
KGM = Kilogram
MTQ = Cubic metre
MWH = Megawatt hour (1000 kWh)
Segment Notes:
This segment is used to indicate the quantity tested for the current line item. Example: QTY+40E:400' Dependency Notes : DE 6411: This DE is only used if the product which was tested is a variable quantity product.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |