EANCOM PART II |  | 1997-07-01

OSTRPT | - | Order status report | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 13 |  | Next Segment

SG3 | - | C | 1000 | - | DOC-DTM-SG4-SG5
SG4 | - | C | 5 | - | STS-DTM-PCD-NAD
PCD | - | C | 1 | - | Percentage details
Function:
To specify percentage information.
EDIFACT
EAN
*
Description |
C501
PERCENTAGE DETAILS
M |
M
| 5245
| Percentage qualifier |
M |  | an..3
M
9E = Percentage of order (EAN Code)
10E = Transport weight percentage completed (EAN Code)
11E = Transport cube percentage completed (EAN Code)
| 5482
| Percentage |
C |  | n..10
R
| 5249
| Percentage basis, coded |
C |  | an..3
N
| 1131
| Code list qualifier |
C |  | an..3
N
| 3055
| Code list responsible agency, coded |
C |  | an..3
R
*
9 = EAN (International Article Numbering association)
Segment Notes:
This segment is used to specify percentage complete figures related to the current order being reported upon. Codes 10E and 11E in data element 5245 are to be used only when weights or cubes in transport or movement orders are being reported. Whether this PCD relates to total LIN or total QTY must be agreed bilaterally. Example : PCD+9E:40:::9' The order is 40% completed.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |