EANCOM PART II |  | 1997-07-01

GENRAL | - | General purpose message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 1 |  | Next Segment

UNH | - | M | 1 | - | MESSAGE HEADER
Function:
To head, identify and specify a message.
EDIFACT
EAN
*
Description |
0062
Message reference number
M |  | an..14
M
Senders unique message reference. Sequence number of messages in the interchange. DE 0062 in the UNT will have the same value. This number is generated by the sender.
S009
MESSAGE IDENTIFIER
M |
M
| 0065
| Message type identifier |
M |  | an..6
M
*
GENRAL = General purpose message
| 0052
| Message type version number |
M |  | an..3
M
*
D = Draft directory
| 0054
| Message type release number |
M |  | an..3
M
*
96A = Version 96A
| 0051
| Controlling agency |
M |  | an..2
M
*
UN = UN/ECE/TRADE/WP.4, United Nations Standard Messages (UNSM)
| 0057
| Association assigned code |
C |  | an..6
R
*
EAN003 = EAN Version control number. |
0068
Common access reference
C |  | an..35
N
S010
STATUS OF THE TRANSFER
C |
N
| 0070
| Sequence message transfer number |
M |  | n..2
| 0073
| First/last sequence message transfer indication |
C |  | a1
Segment Notes:
This segment is used to head, identify and specify a message. DE's 0065, 0052, 0054, and 0051: Indicate that the message is a UNSM General message based on the D.96A directory under the control of the United Nations. DE 0057: Indicates that the message is the EANCOM version 003 of the General message. Example : UNH+ME000001+GENRAL:D:96A:UN:EAN003'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |