EANCOM PART II |  | 1997-07-01

HANMOV | - | Cargo/goods handling and movement message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 24 |  | Next Segment

SG7 | - | C | 99 | - | LIN-PIA-IMD-HAN-SG8-QTY-DTM-FTX-SG10-SG11
SG11 | - | C | 99 | - | PAC-MEA-QTY-SG12
SG12 | - | C | 9 | - | PCI-GIN
GIN | - | C | 9 | - | Goods identity number
Function:
To give specific identification numbers, either as single numbers or ranges.
EDIFACT
EAN
*
Description |
7405
Identity number qualifier
M |  | an..3
M
BJ = Serial shipping container code
BX = Batch number
EU = EAN / UPC number (EAN Code)
C208
IDENTITY NUMBER RANGE
M |
M
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
O
C208
IDENTITY NUMBER RANGE
C |
O
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
O
C208
IDENTITY NUMBER RANGE
C |
O
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
O
C208
IDENTITY NUMBER RANGE
C |
O
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
O
C208
IDENTITY NUMBER RANGE
C |
O
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
O
Segment Notes:
This segment is used to provide identification numbers relevant to the packaging identified in the PAC segment. In EANCOM it is recommended to use the Serial Shipping Container Code (SSCC) for unique identification of individual transport packages. Example : GIN+BJ+354123450000000014:354123450000000106'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |