EANCOM PART II |  | 1997-07-01

MSCONS | - | Metered services consumption report | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 28 |  | Next Segment

SG5 | - | M | 99999 | - | NAD-SG6
SG6 | - | M | 99999 | - | LOC-DTM-SG7-SG8-SG9
SG9 | - | C | 99999 | - | LIN-PIA-IMD-PRI-NAD-MOA-SG10-SG11
SG11 | - | C | 99 | - | CCI-MEA-DTM
MEA | - | C | 99 | - | Measurements
Function:
To specify physical measurements, including dimension tolerances, weights and counts.
EDIFACT
EAN
*
Description |
6311
Measurement application qualifier
M |  | an..3
M
SV = Specification value
C502
MEASUREMENT DETAILS
C |
O
| 6313
| Measurement dimension, coded |
C |  | an..3
A
AAP = Voltage
AAQ = Power consumption
AAR = Heat dissipation
AAY = Water content
ABJ = Volume
TC = Temperature
ZWA = Waste content
| 6321
| Measurement significance, coded |
C |  | an..3
O
3 = Approximately
4 = Equal to
| 6155
| Measurement attribute, coded |
C |  | an..3
O
| 6154
| Measurement attribute |
C |  | an..70
N
C174
VALUE/RANGE
C |
R
| 6411
| Measure unit qualifier |
M |  | an..3
M
001 = Barrel (205 litres, 45 gallons) (EAN Code)
002 = Degree days (EAN Code)
003 = Gigacaloric (EAN Code)
004 = Megajoule per cubic metre (EAN Code)
GJO = Gigajoule
GLI = Gallon (4,546092 dm3)
GWH = Gigawatt-hour (1 million kW/h)
KHZ = Kilohertz
KJO = Kilojoule
KVT = Kilovolt
KWH = Kilowatt hour
VLT = Volt
| 6314
| Measurement value |
C |  | n..18
O
| 6162
| Range minimum |
C |  | n..18
O
| 6152
| Range maximum |
C |  | n..18
O
| 6432
| Significant digits |
C |  | n..2
O
7383
Surface/layer indicator, coded
C |  | an..3
N
Segment Notes:
This segment is used to specify any measurements related to the currently identified product characteristic class. Example : MEA+SV+AAP+VLT:2000'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |