EANCOM PART II |  | 1997-07-01

PRICAT | - | Price/sales catalogue message | VERSION | 006

5. Segments Layout |

Previous Segment |  | Segment number: | 102 |  | Next Segment

SG16 | - | C | 1000 | - | PGI-DTM-QTY-ALI-FTX-SG17-SG18-SG19-SG20-SG26-SG29-SG30-SG31-SG32-SG33
SG33 | - | C | 999999 | - | LIN-PIA-IMD-MEA-QTY-HAN-ALI-DTM-RFF-LOC-FTX-SG35-SG37-SG38-SG44-SG45
SG44 | - | C | 10 | - | PAC-MEA-HAN
HAN | - | C | 5 | - | Handling instructions
Function:
To specify handling and where necessary, notify hazards.
EDIFACT
EAN
*
Description |
C524
HANDLING INSTRUCTIONS
C |
R
| 4079
| Handling instructions, coded |
C |  | an..3
R
BIG = Outsized
CRU = Crushable (EAN Code)
DAE = Dangerous article (EAN Code)
EAT = Foodstuffs
FTD = Frost danger (EAN Code)
HWC = Handle with care (EAN Code)
LYP = Lying
PSC = Pest controlling (EAN Code)
RFS = Flammable solid
SSN = Smell sensitive (EAN Code)
STK = Stackable
STR = Stacking restricted (EAN Code)
TDR = Transit or cross docking delivery
UPR = Up right/standing
UST = Unstackable (EAN Code)
| 1131
| Code list qualifier |
C |  | an..3
N
| 3055
| Code list responsible agency, coded |
C |  | an..3
D
*
9 = EAN (International Article Numbering association)
2 = CEC (Commission of the European Communities)
| 4078
| Handling instructions |
C |  | an..70
O
C218
HAZARDOUS MATERIAL
C |
O
| 7419
| Hazardous material class code, identification |
C |  | an..4
O
| 1131
| Code list qualifier |
C |  | an..3
O
| 3055
| Code list responsible agency, coded |
C |  | an..3
O
Segment Notes:
This segment is used to specify the handling instructions related to the package identified in the PAC segment. Example : HAN+EAT' HAN+HWC::9' Dependency Notes : DE 3055: This data element must be used when using any of the EAN specific codes in data element 4079.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |