EANCOM PART II |  | 1997-07-01

CONTRL | - | Control message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 3 |  | Next Segment

SG1 | - | C | 999999 | - | UCM-SG2
UCM | - | M | 1 | - | MESSAGE RESPONSE
Function:
To identify a message in the subject interchange, to indicate that message's acknowledgement or rejection (action taken), and to identify any error related to the UNH and UNT segments.
EDIFACT
EAN
*
Description |
0062
Message reference number
M |  | an..14
M
S009
MESSAGE IDENTIFIER
M |
M
| 0065
| Message type identifier |
M |  | an..6
M
| 0052
| Message type version number |
M |  | an..3
M
| 0054
| Message type release number |
M |  | an..3
M
| 0051
| Controlling agency |
M |  | an..2
M
| 0057
| Association assigned code |
C |  | an..6
R
0083
Action, coded
M |  | an..3
M
4 = Rejected - this level and all lower levels
7 = This level acknowledged, next level acknowledged if not explicitly rejected
0085
Syntax error, coded
C |  | an..3
D
*
12 = Invalid value
13 = Missing
14 = Value not supported in this position
15 = Not supported in this position
16 = Too many constituents
17 = No agreement
18 = Unspecified error
21 = Invalid character(s)
22 = Invalid service character(s)
23 = Unknown interchange sender
25 = Test indicator not supported
26 = Duplicate detected
27 = Security function not supported
28 = References do not match
29 = Control count does not match number of instances received
30 = Functional groups and messages mixed
31 = More than one message type in group
34 = Nesting indicator not allowed
37 = Invalid type of character(s)
39 = Data element too long
40 = Data element too short
0013
Segment tag, coded
C |  | a3
D
S011
DATA ELEMENT POSITION
C |
D
| 0098
| Erroneous data element position in segment |
M |  | n..3
M
| 0104
| Erroneous component data element position |
C |  | n..3
O
Segment Notes:
This segment is used to identify specific messages within the interchange identified in the previous UCI segment. This segment is similar in layout to the UNH segment (data elements 0062 to 0057 inclusive) and should contain the same information as that contained in the UNH segment. DE's 0083 and 0085: These data elements are used to indicate the status of the message and in cases where errors are present to identify the error. DE's 0013, S011: If there are errors in the UNH or UNT segments the segment in question and the position of the error in the segment may be identified in these data elements. DE 0098: The numerical count position of the simple or composite data element in error. The segment tag and each simple and composite data element position number within the segment. DE 0104: The numerical count position of the component data element in error. Each component data element position defined in the composite data element description shall cause the count to be incremented. Example : UCM+ME002341+INVOIC:D:96A:UN:EAN008+4+13+UNH+2' Message reference ME002341, an INVOIC message, has been rejected because the mandatory data element 0062 has not been included in the UNH segment position 2. Dependency Notes : Data elements 0085, 0013 and S011 are only used when errors are being reported.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |