EANCOM PART II |  | 1997-07-01

RETINS | - | Returns instruction | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 29 |  | Next Segment

SG11 | - | C | 9999 | - | LIN-PIA-IMD-MEA-DTM-QTY-LOC-MOA-SG12-SG13-SG16-SG18
SG16 | - | C | 9 | - | PAC-SG17
PAC | - | M | 1 | - | Package
Function:
To describe the number and type of packages/physical units.
EDIFACT
EAN
*
Description |
7224
Number of packages
C |  | n..8
O
C531
PACKAGING DETAILS
C |
O
| 7075
| Packaging level, coded |
C |  | an..3
N
| 7233
| Packaging related information, coded |
C |  | an..3
O
| 7073
| Packaging terms and conditions, coded |
C |  | an..3
N
C202
PACKAGE TYPE
C |
R
| 7065
| Type of packages identification |
C |  | an..17
A
09 = Returnable pallet (EAN Code)
BX = Box
CR = Crate
PK = Package
| 1131
| Code list qualifier |
C |  | an..3
O
| 3055
| Code list responsible agency, coded |
C |  | an..3
O
9 = EAN (International Article Numbering association)
| 7064
| Type of packages |
C |  | an..35
O
C402
PACKAGE TYPE IDENTIFICATION
C |
N
| 7077
| Item description type, coded |
M |  | an..3
| 7064
| Type of packages |
M |  | an..35
| 7143
| Item number type, coded |
C |  | an..3
| 7064
| Type of packages |
C |  | an..35
| 7143
| Item number type, coded |
C |  | an..3
C532
RETURNABLE PACKAGE DETAILS
C |
N
| 8395
| Returnable package freight payment responsibility, coded |
C |  | an..3
| 8393
| Returnable package load contents, coded |
C |  | an..3
Segment Notes:
This segment is used to provide packaging information for the line item being returned. Example : PAC+++CR'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |