EANCOM PART II |  | 1997-07-01

MSCONS | - | Metered services consumption report | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 26 |  | Next Segment

SG5 | - | M | 99999 | - | NAD-SG6
SG6 | - | M | 99999 | - | LOC-DTM-SG7-SG8-SG9
SG9 | - | C | 99999 | - | LIN-PIA-IMD-PRI-NAD-MOA-SG10-SG11
SG10 | - | M | 9999 | - | QTY-DTM
DTM | - | C | 9 | - | Date/time/period
Function:
To specify date, and/or time, or period.
EDIFACT
EAN
*
Description |
C507
DATE/TIME/PERIOD
M |
M
| 2005
| Date/time/period qualifier |
M |  | an..3
M
*
263 = Invoicing period
273 = Validity period
356 = Sales date, and or time, and or period
367 = Previous meter reading date
368 = Latest meter reading date
44E = Connection date/time (EAN Code)
45E = Disconnection date/time (EAN Code)
| 2380
| Date/time/period |
C |  | an..35
R
| 2379
| Date/time/period format qualifier |
C |  | an..3
R
204 = CCYYMMDDHHMMSS
20E = CCYYMMDDHHMM-CCYYMMDDHHMM (EAN Code)
Segment Notes:
This segment is used to specify any dates and or times related to the quantity specified in the previous QTY segment. DE 2005: Codes 44E and 45E should only be used to indicate the date/time of connection and disconnect of a telephone call. Example : DTM+367:19970102:102'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |