EANCOM PART II |  | 1997-07-01

HANMOV | - | Cargo/goods handling and movement message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 16 |  | Next Segment

SG7 | - | C | 99 | - | LIN-PIA-IMD-HAN-SG8-QTY-DTM-FTX-SG10-SG11
QTY | - | C | 9 | - | Quantity
Function:
To specify a pertinent quantity.
EDIFACT
EAN
*
Description |
C186
QUANTITY DETAILS
M |
M
| 6063
| Quantity qualifier |
M |  | an..3
M
1 = Discrete quantity
52 = Quantity per pack
17E = Number of units in lower packaging or configuration level (EAN Code)
45E = Number of units in higher packaging or configuration level (EAN Code)
| 6060
| Quantity |
M |  | n..15
M
| 6411
| Measure unit qualifier |
C |  | an..3
D
KGM = Kilogram
Segment Notes:
This segment is used to specify quantities related to the current line item. Example : QTY+52:40' Dependency Notes : DE 6411: This DE is only used if the current line item is of variable quantity.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |