EANCOM PART III DATA ELEMENT & CODE SETS DIRECTORY |  | 1997-07-01

Previous Data Element |  | Next Data Element

0073
| First/last sequence message transfer indication
| Indication used for the first and last message in a sequence of the same type of message relating to the same topic.

| C
= | Creation
| First transmission of a number of transfers of the same message.
| F
= | Final
| Last transmission of a number of transfers of the same message.

Previous Data Element |  | Next Data Element

(c) Copyright EAN 1997 |