EANCOM PART II |  | 1997-07-01

QALITY | - | Quality data message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 22 |  | Next Segment

SG5 | - | C | 200 | - | LIN-PIA-IMD-MEA-DTM-QTY-FTX-SG6-SG7-SG12
SG12 | - | C | 200 | - | CCI-SG14
SG14 | - | C | 999 | - | MEA
MEA | - | M | 1 | - | Measurements
Function:
To specify physical measurements, including dimension tolerances, weights and counts.
EDIFACT
EAN
*
Description |
6311
Measurement application qualifier
M |  | an..3
M
MV = Measured value (EAN Code)
TR = Test result
C502
MEASUREMENT DETAILS
C |
A
| 6313
| Measurement dimension, coded |
C |  | an..3
A
AAE = Item gross weight AAO = Humidity AAP = Voltage AAR = Heat dissipation ENE = Energy efficiency (EAN Code) TC = Temperature |
| 6321
| Measurement significance, coded |
C |  | an..3
O
| 6155
| Measurement attribute, coded |
C |  | an..3
N
| 6154
| Measurement attribute |
C |  | an..70
N
C174
VALUE/RANGE
C |
R
| 6411
| Measure unit qualifier |
M |  | an..3
M
CEL = Degree celsius
LTR = Litre (1 dm3)
MWH = Megawatt hour (1000 kWh)
VLT = Volt
| 6314
| Measurement value |
C |  | n..18
O
| 6162
| Range minimum |
C |  | n..18
O
| 6152
| Range maximum |
C |  | n..18
O
| 6432
| Significant digits |
C |  | n..2
N
7383
Surface/layer indicator, coded
C |  | an..3
N
Segment Notes:
This segment is used to provide test measurement data related to the current line item. Example : MEA+MV+TC+CEL::40:110' The test was carried out using temperatures in the range of 40 to 110 degrees celsius. MEA+TR+AAR+++MWH:0.5' The heat dissipated during the test was 0.5 megawatt hours.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |