EANCOM PART II |  | 1997-07-01

PRODAT | - | Product data message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 48 |  | Next Segment

SG8 | - | M | 999 | - | LIN-PIA-DTM-MEA-HAN-DOC-FTX-PGI-SG9-SG10-SG12-SG14-SG15-SG16-SG17-SG19-SG20-SG21
SG21 | - | C | 999 | - | HYN-QTY-SG23
SG23 | - | C | 99 | - | CCI-CAV-MEA
MEA | - | C | 10 | - | Measurements
Function:
To specify physical measurements, including dimension tolerances, weights and counts.
EDIFACT
EAN
*
Description |
6311
Measurement application qualifier
M |  | an..3
M
PD = Physical dimensions (product ordered)
SV = Specification value
C502
MEASUREMENT DETAILS
C |
A
| 6313
| Measurement dimension, coded |
C |  | an..3
A
AAA = Unit net weight
DI = Diameter
DP = Depth
HT = Height dimension
LN = Length dimension
TH = Thickness
| 6321
| Measurement significance, coded |
C |  | an..3
O
3 = Approximately
4 = Equal to
| 6155
| Measurement attribute, coded |
C |  | an..3
O
| 6154
| Measurement attribute |
C |  | an..70
N
C174
VALUE/RANGE
C |
R
| 6411
| Measure unit qualifier |
M |  | an..3
M
CMT = Centimetre
FOT = Foot (0,3048 m)
GRM = Gram
MMT = Millimetre
MTR = Metre
PCD = Percentage (EAN Code)
YRD = Yard (0,9144 m)
| 6314
| Measurement value |
C |  | n..18
O
| 6162
| Range minimum |
C |  | n..18
O
| 6152
| Range maximum |
C |  | n..18
O
| 6432
| Significant digits |
C |  | n..2
N
7383
Surface/layer indicator, coded
C |  | an..3
N
Segment Notes:
This segment is used to specify any measurements related to the currently identified hierarchy characteristic class. Example : MEA+PD+LN:4+MTR:8'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |