EANCOM PART II |  | 1997-07-01

PRICAT | - | Price/sales catalogue message | VERSION | 006

5. Segments Layout |

Previous Segment |  | Segment number: | 68 |  | Next Segment

SG16 | - | C | 1000 | - | PGI-DTM-QTY-ALI-FTX-SG17-SG18-SG19-SG20-SG26-SG29-SG30-SG31-SG32-SG33
SG32 | - | C | 10 | - | PAC-MEA
MEA | - | C | 10 | - | Measurements
Function:
To specify physical measurements, including dimension tolerances, weights and counts.
EDIFACT
EAN
*
Description |
6311
Measurement application qualifier
M |  | an..3
M
PD = Physical dimensions (product ordered)
SO = Storage limitation
TL = Transportation equipment limitations
C502
MEASUREMENT DETAILS
C |
A
| 6313
| Measurement dimension, coded |
C |  | an..3
A
ADX = Transport container actual filling weight
ADZ = Declared net weight
AEA = Loading height
AEB = Stacking height
HT = Height dimension
LAY = Number of layers (EAN Code)
LN = Length dimension
ULY = Number of units per layer (EAN Code)
WD = Width dimension
| 6321
| Measurement significance, coded |
C |  | an..3
O
3 = Approximately
4 = Equal to
| 6155
| Measurement attribute, coded |
C |  | an..3
N
| 6154
| Measurement attribute |
C |  | an..70
N
C174
VALUE/RANGE
C |
R
| 6411
| Measure unit qualifier |
M |  | an..3
M
KGM = Kilogram
| 6314
| Measurement value |
C |  | n..18
R
| 6162
| Range minimum |
C |  | n..18
O
| 6152
| Range maximum |
C |  | n..18
O
| 6432
| Significant digits |
C |  | n..2
N
7383
Surface/layer indicator, coded
C |  | an..3
N
Segment Notes:
This segment is used to provide measurement information related to the packaging details for the entire product group. Example: PAC+PD+HT+MMT:600' PAC+PD+LN+MMT:300' PAC+PD+WD+MMT:200' Physical dimensions of the packaging (600m x 300m x 200m)

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |