EANCOM PART II |  | 1997-07-01

IFTMAN | - | Arrival notice message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 32 |  | Next Segment

SG18 | - | C | 999 | - | GID-TMP-RNG-FTX-SG19-SG20-SG21-SG22-SG23-SG27-SG30
SG30 | - | C | 9 | - | DGS-FTX-SG31-SG32
DGS | - | M | 1 | - | Dangerous goods
Function:
To identify dangerous goods.
EDIFACT
EAN
*
Description |
8273
Dangerous goods regulations, coded
C |  | an..3
R
ADR = European agreement regarding the total carriage of dangerous goods
CFR = 49 code of federal regulations
C205
HAZARD CODE
C |
O
| 8351
| Hazard code identification |
M |  | an..7
M
| 8078
| Hazard substance/item/page number |
C |  | an..7
O
| 8092
| Hazard code version number |
C |  | an..10
O
C234
UNDG INFORMATION
C |
O
| 7124
| UNDG number |
C |  | n4
O
| 7088
| Dangerous goods flashpoint |
C |  | an..8
O
C223
DANGEROUS GOODS SHIPMENT FLASHPOINT
C |
O
| 7106
| Shipment flashpoint |
C |  | n3
O
| 6411
| Measure unit qualifier |
C |  | an..3
O
8339
Packing group, coded
C |  | an..3
O
1 = Great danger
2 = Medium danger
3 = Minor danger
8364
EMS number
C |  | an..6
O
8410
MFAG
C |  | an..4
O
8126
Trem card number
C |  | an..10
O
C235
HAZARD IDENTIFICATION
C |
N
| 8158
| Hazard identification number, upper part |
C |  | an..4
| 8186
| Substance identification number, lower part |
C |  | an4
C236
DANGEROUS GOODS LABEL
C |
N
| 8246
| Dangerous goods label marking |
C |  | an..4
| 8246
| Dangerous goods label marking |
C |  | an..4
| 8246
| Dangerous goods label marking |
C |  | an..4
Segment Notes:
This segment is used to indicate whether the goods item in the arriving consignment contains any dangerous goods. Example : DGS+ADR+3B+1178+21.0:CEL' Dangerous goods according to the ADR regulation 3B for extremely flammable liquids with a flashpoint of 21 degrees celsius and a UN number 1178.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |