EANCOM PART II |  | 1997-07-01

IFTMBF | - | Firm booking message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 9 |  | Next Segment

SG3 | - | C | 99 | - | RFF-DTM
RFF | - | M | 1 | - | Reference
Function:
To specify a reference.
EDIFACT
EAN
*
Description |
C506
REFERENCE
M |
M
| 1153
| Reference qualifier |
M |  | an..3
M
BN = Booking reference number
CT = Contract number
CU = Consignor's reference number
PFB = Firm booking reference number (EAN Code)
| 1154
| Reference number |
C |  | an..35
R
| 1156
| Line number |
C |  | an..6
N
| 4000
| Reference version number |
C |  | an..35
N
Segment Notes:
This segment is used to specify references relating to the booking. DE 1153: Code value 'PFB' is only used when codes values 1 (Cancellation) or 5 (Replacement) are used in data element 1225 of the BGM segment. The code value 'CU' is the common reference number for the consignment which is used in all transport messages (IFTMIN, IFTMAN, etc). Example : RFF+CT:76214'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |