EANCOM PART II |  | 1997-07-01

QUOTES | - | Quote message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 21 |  | Next Segment

SG27 | - | M | 200000 | - | LIN-PIA-IMD-MEA-QTY-ALI-DTM-FTX-SG29-SG31-SG32-SG34-SG39-SG46-SG52-SG54
MEA | - | C | 5 | - | Measurements
Function:
To specify physical measurements, including dimension tolerances, weights and counts.
EDIFACT
EAN
*
Description |
6311
Measurement application qualifier
M |  | an..3
M
PD = Physical dimensions (product ordered)
SO = Storage limitation
TL = Transportation equipment limitations
C502
MEASUREMENT DETAILS
C |
A
| 6313
| Measurement dimension, coded |
C |  | an..3
A
AAA = Unit net weight
AAF = Net net weight
HT = Height dimension
LN = Length dimension
WD = Width dimension
| 6321
| Measurement significance, coded |
C |  | an..3
O
3 = Approximately
4 = Equal to
| 6155
| Measurement attribute, coded |
C |  | an..3
N
| 6154
| Measurement attribute |
C |  | an..70
N
C174
VALUE/RANGE
C |
R
| 6411
| Measure unit qualifier |
M |  | an..3
M
CEL = Degree Celsius
KGM = Kilogram
MMT = Millimetre
| 6314
| Measurement value |
C |  | n..18
O
| 6162
| Range minimum |
C |  | n..18
O
| 6152
| Range maximum |
C |  | n..18
O
| 6432
| Significant digits |
C |  | n..2
O
7383
Surface/layer indicator, coded
C |  | an..3
N
Segment Notes:
This segment is used to indicate measurements or limitations of the current line item. Example : MEA+PD+HT+MMT:500' MEA+PD+LN+MMT:200' MEA+PD+WD+MMT:100' Product with dimensions 500mm x 200mm x 100mm

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |