EANCOM PART III DATA ELEMENT & CODE SETS DIRECTORY |  | 1997-07-01

Previous Data Element |  | Next Data Element

7075
| Packaging level, coded
| Indication of level of packaging specified.

+ | 1
= | Inner
| Level of packing, if it exists, that is immediately subordinate to the intermediate packaging level.
+ | 2
= | Intermediate
| Level of packaging, if it exists, that is immediately subordinate to the outer packaging level.
+ | 3
= | Outer
| For packed merchandise, outermost level of packaging for a shipment.

Previous Data Element |  | Next Data Element

(c) Copyright EAN 1997 |