EANCOM PART II |  | 1997-07-01

IFTMAN | - | Arrival notice message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 19 |  | Next Segment

SG18 | - | C | 999 | - | GID-TMP-RNG-FTX-SG19-SG20-SG21-SG22-SG23-SG27-SG30
TMP | - | C | 1 | - | Temperature
Function:
To specify the temperature setting.
EDIFACT
EAN
*
Description |
6245
Temperature qualifier
M |  | an..3
M
*
2 = Transport temperature
C239
TEMPERATURE SETTING
C |
R
| 6246
| Temperature setting |
C |  | n3
O
| 6411
| Measure unit qualifier |
C |  | an..3
O
CEL = Degree celsius
FAH = Degree fahrenheit
KEL = Kelvin
Segment Notes:
This segment is used to specify transport temperature settings related to the current goods item. Example : TMP+2+040:CEL'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |