EANCOM PART II |  | 1997-07-01

PRODAT | - | Product data message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 42 |  | Next Segment

SG8 | - | M | 999 | - | LIN-PIA-DTM-MEA-HAN-DOC-FTX-PGI-SG9-SG10-SG12-SG14-SG15-SG16-SG17-SG19-SG20-SG21
SG20 | - | C | 5 | - | PAC-MEA-HAN-PCI
HAN | - | C | 5 | - | Handling instructions
Function:
To specify handling and where necessary, notify hazards.
EDIFACT
EAN
*
Description |
C524
HANDLING INSTRUCTIONS
C |
O
| 4079
| Handling instructions, coded |
C |  | an..3
O
BIG = Outsized
CRU = Crushable (EAN Code)
EAT = Foodstuffs
HWC = Handle with care (EAN Code)
STR = Stacking restricted (EAN Code)
UST = Unstackable (EAN Code)
| 1131
| Code list qualifier |
C |  | an..3
N
| 3055
| Code list responsible agency, coded |
C |  | an..3
D
*
9 = EAN (International Article Numbering association)
| 4078
| Handling instructions |
C |  | an..70
O
C218
HAZARDOUS MATERIAL
C |
O
| 7419
| Hazardous material class code, identification |
C |  | an..4
O
| 1131
| Code list qualifier |
C |  | an..3
O
| 3055
| Code list responsible agency, coded |
C |  | an..3
O
Segment Notes:
This segment is used to provide handling instructions relevant to the packaging unit described in the PAC segment. Example : HAN+CRU::9' Dependency Notes : DE 3055: This data element is only used when EAN codes, i.e. CRU, UST, HWC, etc, are used in data element 4079.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |