EANCOM PART II |  | 1997-07-01

IFTMIN | - | Instruction message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 50 |  | Next Segment

SG37 | - | C | 999 | - | EQD-MEA-DIM-SEL-SG39
MEA | - | C | 9 | - | Measurements
Function:
To specify physical measurements, including dimension tolerances, weights and counts.
EDIFACT
EAN
*
Description |
6311
Measurement application qualifier
M |  | an..3
M
AAE = Measurement
C502
MEASUREMENT DETAILS
C |
A
| 6313
| Measurement dimension, coded |
C |  | an..3
A
G = Gross weight
T = Tare weight
| 6321
| Measurement significance, coded |
C |  | an..3
O
3 = Approximately
4 = Equal to
| 6155
| Measurement attribute, coded |
C |  | an..3
O
| 6154
| Measurement attribute |
C |  | an..70
N
C174
VALUE/RANGE
C |
R
| 6411
| Measure unit qualifier |
M |  | an..3
M
KGM = Kilogram
TNE = Metric ton (1000kg)
| 6314
| Measurement value |
C |  | n..18
O
| 6162
| Range minimum |
C |  | n..18
O
| 6152
| Range maximum |
C |  | n..18
O
| 6432
| Significant digits |
C |  | n..2
O
7383
Surface/layer indicator, coded
C |  | an..3
N
Segment Notes:
This segment is used to specify the physical dimensions including tolerances of the equipment identified in the preceding EQD segment. Example : MEA+AAE+G+TNE:5622'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |