EANCOM PART II |  | 1997-07-01

DELFOR | - | Delivery schedule message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 26 |  | Next Segment

SG18 | - | C | 9999 | - | IMD-PIA-SG19-SG20-SG22-SG24
SG20 | - | C | 50 | - | QTY-SCC-DTM
SCC | - | C | 1 | - | Scheduling conditions
Function:
To specify scheduling conditions.
EDIFACT
EAN
*
Description |
4017
Delivery plan status indicator, coded
M |  | an..3
M
1 = Firm
4 = Planning/forecast
10 = Immediate
10E = Promised (EAN Code)
4493
Delivery requirements, coded
C |  | an..3
O
DA = Do not deliver after
DB = Do not deliver before
DD = Deliver on date
P2 = Ship as soon as possible
SC = Ship complete order
C329
PATTERN DESCRIPTION
C |
O
| 2013
| Frequency, coded |
C |  | an..3
O
M = Monthly (calendar months)
Q = Quarterly (calendar quarters)
W = Weekly
Y = Daily
| 2015
| Despatch pattern, coded |
C |  | an..3
O
10 = Monday through Friday
11 = Monday through Saturday
13 = Monday
14 = Tuesday
15 = Wednesday
16 = Thursday
17 = Friday
18 = Saturday
| 2017
| Despatch pattern timing, coded |
C |  | an..3
O
D = A.M.
E = P.M.
H = 24 hour clock
Segment Notes:
This segment is used to specify the type and status of the schedule being given, and optionally defining a pattern to be established, e.g., firm or proposed delivery schedule for a weekly pattern. Example : SCC+1+SC+W'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |