EANCOM PART II |  | 1997-07-01

ORDERS | - | Purchase order message | VERSION | 008

5. Segments Layout |

Previous Segment |  | Segment number: | 42 |  | Next Segment

SG25 | - | C | 200000 | - | LIN-PIA-IMD-MEA-QTY-DTM-MOA-GIN-QVR-FTX-SG28-SG29-SG30-SG33-SG34-SG35-SG39-SG45
MEA | - | C | 5 | - | Measurements
Function:
To specify physical measurements, including dimension tolerances, weights and counts.
EDIFACT
EAN
*
Description |
6311
Measurement application qualifier
M |  | an..3
M
PD = Physical dimensions (product ordered)
C502
MEASUREMENT DETAILS
C |
A
| 6313
| Measurement dimension, coded |
C |  | an..3
A
DI = Diameter
DP = Depth
ID = Inside diameter
HT = Height dimension
LN = Length dimension
OD = Outside diameter
TH = Thickness
| 6321
| Measurement significance, coded |
C |  | an..3
O
3 = Approximately
4 = Equal to
| 6155
| Measurement attribute, coded |
C |  | an..3
O
| 6154
| Measurement attribute |
C |  | an..70
N
C174
VALUE/RANGE
C |
R
| 6411
| Measure unit qualifier |
M |  | an..3
M
CMT = Centimetre
FOT = Foot (0,3048 m)
MMT = Millimetre
MTK = Square metre
MTR = Metre
YRD = Yard (0,9144 m)
| 6314
| Measurement value |
C |  | n..18
O
| 6162
| Range minimum |
C |  | n..18
O
| 6152
| Range maximum |
C |  | n..18
O
| 6432
| Significant digits |
C |  | n..2
O
7383
Surface/layer indicator, coded
C |  | an..3
N
Segment Notes:
This segment is used to specify the actual physical dimensions of the product being ordered where that product is sold in variable lengths or volumes. This segment must be used in conjunction with the LIN segment for the precise identification of the ordered product. Example: MEA+PD+LN:4+MTR:4.5' The precise length of the product identified by the EAN article number 5412345111115 is 4.5 metres.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |