EANCOM PART II |  | 1997-07-01

RECADV | - | Receiving advice message | VERSION | 003

5. Segments Layout |

Previous Segment |  | Segment number: | 26 |  | Next Segment

SG16 | - | C | 9999 | - | CPS-SG17-SG22
SG22 | - | C | 9999 | - | LIN-PIA-QTY-QVR-DTM-SG28-SG29
SG29 | - | C | 9999 | - | PCI-QTY-QVR-SG31
SG31 | - | C | 10 | - | GIN
GIN | - | M | 1 | - | Goods identity number
Function:
To give specific identification numbers, either as single numbers or ranges.
EDIFACT
EAN
*
Description |
7405
Identity number qualifier
M |  | an..3
M
BJ = Serial shipping container code
C208
IDENTITY NUMBER RANGE
M |
M
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
O
C208
IDENTITY NUMBER RANGE
C |
O
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
O
C208
IDENTITY NUMBER RANGE
C |
O
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
O
C208
IDENTITY NUMBER RANGE
C |
O
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
O
C208
IDENTITY NUMBER RANGE
C |
O
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
O
Segment Notes:
This segment is used to provide the Serial Shipping Container Code marked on the packaging of the current line item. DE C208: If a sequential series of identity numbers is provided (e.g., 1 up to and including 10) only one repetition of the C208 composite is needed with the first repetition of 7402 specifying the numerically smaller identity number (e.g., 1) and the second repetition the larger identity number (e.g., 10). If identity numbers are not sequential and part of a series (e.g., 1, 3, and 10) then a separate C208 and DE 7402 must be used for each identity number. Within internal applications, users may provide a range of Serial Shipping Container Codes using one repetition of C208 (as described above) by transmitting a 17 digit SSCC and calculating the check digit within the application. The full 18 digit Serial Shipping Container Code (not in sequence due to check digit algorithm) must be transmitted using a separate C208 composite in open trade applications. In EANCOM it is recommended to use the Serial Shipping Container Code (SSCC) for unique identification of individual transport packages. Example : GIN+BJ+354123450000000014'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |