EANCOM PART II |  | 1997-07-01

HANMOV | - | Cargo/goods handling and movement message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 19 |  | Next Segment

SG7 | - | C | 99 | - | LIN-PIA-IMD-HAN-SG8-QTY-DTM-FTX-SG10-SG11
SG10 | - | C | 9 | - | RFF
RFF | - | M | 1 | - | Reference
Function:
To specify a reference.
EDIFACT
EAN
*
Description |
C506
REFERENCE
M |
M
| 1153
| Reference qualifier |
M |  | an..3
M
CR = Customer reference number
CT = Contract number
ON = Order number (buyer)
PK = Packing list number
VN = Order number (supplier)
| 1154
| Reference number |
C |  | an..35
R
| 1156
| Line number |
C |  | an..6
O
| 4000
| Reference version number |
C |  | an..35
N
Segment Notes:
This segment is used to provide references specific to the line item. References specified here override any global references provided in the heading section of the cargo/goods handling and movement message when the same qualifier is used. Example : RFF+PK:8306'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |