EANCOM PART II |  | 1997-07-01

INSDES | - | Instruction to despatch | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 5 |  | Next Segment

SG1 | - | C | 9 | - | RFF-DTM
RFF | - | M | 1 | - | Reference
Function:
To specify a reference.
EDIFACT
EAN
*
Description |
C506
REFERENCE
M |
M
| 1153
| Reference qualifier |
M |  | an..3
M
AAJ = Delivery order number
AAN = Delivery schedule number
AAU = Despatch note number
CNE = Consolidated reference number (EAN Code)
CT = Contract number
CU = Consignor's reference number
ECN = External consolidation reference number (EAN Code)
ERC = External recap reference number (EAN Code)
HN = Handling and movement reference number (EAN Code)
IDR = Instruction to despatch reference number (EAN Code)
IP = Import licence number
ON = Order number (buyer)
RCE = Recap number (EAN Code)
| 1154
| Reference number |
C |  | an..35
R
| 1156
| Line number |
C |  | an..6
N
| 4000
| Reference version number |
C |  | an..35
N
Segment Notes:
This segment is used to specify references relating to the instruction to despatch. DE 1153: When data element 1225 in the BGM segment is used with the code values '1, Cancellation' or '5, Replace' then the code value 'IDR' must be included to provide a link with a previous instruction to despatch. Example : RFF+CT:52114'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |