EANCOM PART II |  | 1997-07-01

PRICAT | - | Price/sales catalogue message | VERSION | 006

5. Segments Layout |

Previous Segment |  | Segment number: | 72 |  | Next Segment

SG16 | - | C | 1000 | - | PGI-DTM-QTY-ALI-FTX-SG17-SG18-SG19-SG20-SG26-SG29-SG30-SG31-SG32-SG33
SG33 | - | C | 999999 | - | LIN-PIA-IMD-MEA-QTY-HAN-ALI-DTM-RFF-LOC-FTX-SG35-SG37-SG38-SG44-SG45
MEA | - | C | 10 | - | Measurements
Function:
To specify physical measurements, including dimension tolerances, weights and counts.
EDIFACT
EAN
*
Description |
6311
Measurement application qualifier
M |  | an..3
M
CME = Price comparison measurement (EAN Code)
PD = Physical dimensions (product ordered)
SO = Storage limitation
C502
MEASUREMENT DETAILS
C |
A
| 6313
| Measurement dimension, coded |
C |  | an..3
A
AAA = Unit net weight
AAF = Net net weight
ABJ = Volume
DLL = Diluted liquid (EAN Code)
DWT = Drained weight (EAN Code)
HT = Height dimension
NUP = Number of units per pallet (EAN Code)
RA = Relative humidity
TC = Temperature
WD = Width dimension
| 6321
| Measurement significance, coded |
C |  | an..3
O
3 = Approximately
4 = Equal to
| 6155
| Measurement attribute, coded |
C |  | an..3
O
42 = Uncontrolled temperature
43 = Chilled
44 = Frozen
45 = Temperature controlled
| 6154
| Measurement attribute |
C |  | an..70
N
C174
VALUE/RANGE
C |
R
| 6411
| Measure unit qualifier |
M |  | an..3
M
CEL = Degree celsius
KGM = Kilogram
MGM = Milligram
04 = small spray
MLT = Millilitre
MMT = Millimetre
P1 = Percentage
PTN = Portion (EAN Code)
ST = Sheet
| 6314
| Measurement value |
C |  | n..18
O
| 6162
| Range minimum |
C |  | n..18
O
| 6152
| Range maximum |
C |  | n..18
O
| 6432
| Significant digits |
C |  | n..2
N
7383
Surface/layer indicator, coded
C |  | an..3
N
Segment Notes:
This segment is used to specify measurements related to the article identified in the LIN segment. Measurements related to the packaging of the article are provided in the MEA segment of the PAC segment group. DE 6313: The code value 'NUP' is used to indicate the total number of units on a pallet by multiplying the number of units per layer by the number of layers on a pallet. Examples: 1. Physical Dimensions of a product without packaging (500mm x 200mm x 100mm) MEA+PD+HT+MMT:500' MEA+PD+LN+MMT:200' MEA+PD+WD+MMT:100' 2. Storage Temperature between 10 and 15 degrees celsius MEA+SO+TC+CEL::10:15' 3. The volume of the product is 100 millilitre's. MEA+PD+VOL+MLT:100' 4. The net weight of the unit is equal to 250 kilograms. MEA+PD+AAA:4+KGM:250'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |