EANCOM PART II |  | 1997-07-01

IFTMAN | - | Arrival notice message | VERSION | 001

4. Segments Description |

Arrival Notice Heading Section
UNH | - | M | 1 | - | MESSAGE HEADER
This segment is used to head, identify and specify a message.
BGM | - | M | 1 | - | Beginning of message
This segment is used to indicate the type and function of a message and to transmit the identifying number.
DTM | - | C | 9 | - | Date/time/period
This segment is used to specify any dates related to the arrival notice message.
TSR | - | C | 9 | - | Transport service requirements
This segment is used to indicate the party responsible for the unloading of the goods from the transport means at the arrival location.
MOA | - | C | 99 | - | Monetary amount
This segment is used to specify monetary values related to the arriving consignment.
FTX | - | C | 99 | - | Free text
This segment is used to provide free form or coded text information related to the entire message.
CNT | - | C | 9 | - | Control total
This segment is used to provide application data for message control purposes.
SG1 | - | C | 99 | - | LOC
A group of segments to specify locations and related date(s)/time(s) which apply to the entire message, e.g. place of transhipment.
LOC | - | M | 1 | - | Place/location identification
This segment is used to identify any locations related to the complete arriving consignment.
SG3 | - | C | 99 | - | RFF-DTM
A group of segments containing a reference and constants which apply to the entire message.
RFF | - | M | 1 | - | Reference
This segment is used to specify references relating to the consignment arriving.
DTM | - | C | 9 | - | Date/time/period
This segment is used to specify any dates related to the previous RFF segment.
SG8 | - | C | 99 | - | TDT-DTM-SG9
A group of segments to indicate details of the movement of goods such as mode and means of transport, locations, departure, and arrival date(s) and time(s).
TDT | - | M | 1 | - | Details of transport
This segment is used to indicate the main carriage transport means, and where necessary, the exact identification of the transport used for the arriving consignment.
DTM | - | C | 9 | - | Date/time/period
This segment is used to specify any dates relating to the transport specified in the previous TDT segment.
SG9 | - | C | 99 | - | LOC
A group of segments to specify a location and date/time related to this leg of transport.
LOC | - | M | 1 | - | Place/location identification
This segment is used to identify any locations related to the transport details previously specified.
SG11 | - | C | 99 | - | NAD-SG12-SG15
A group of segments to identify a party, related references, locations contacts, required documents, and charges to be paid by the party.
NAD | - | M | 1 | - | Name and address
This segment is used to identify the parties involved in the arrival notice message. Identification of the consignor and/or consignee, and/or the carrier or forwarder is mandatory in the arrival notice message.
SG12 | - | C | 9 | - | CTA-COM
A group of segments identifying a contact and its communications related to the party.
CTA | - | M | 1 | - | Contact information
This segment is used to identify department and contact names within the company specified in the NAD segment.
COM | - | C | 9 | - | Communication contact
This segment identifies the communications number and type of communications for the person or department identified in the preceding CTA segment.
SG15 | - | C | 9 | - | RFF
A group of segments to specify a reference related to the party.
RFF | - | M | 1 | - | Reference
This segment is used to identify any references related to the party identified in the NAD segment.
Arrival Notice Detail Section
SG18 | - | C | 999 | - | GID-TMP-RNG-FTX-SG19-SG20-SG21-SG22-SG23-SG27-SG30
A group of segments to describe the goods items for which transport is undertaken.
GID | - | M | 1 | - | Goods item details
This segment is the trigger segment for the detail section of the arrival notice message. It is used to specify the type of packaging for the goods item(s) which are contained in the arriving consignment.
TMP | - | C | 1 | - | Temperature
This segment is used to specify transport temperature settings related to the current goods item.
RNG | - | C | 1 | - | Range details
This segment is used to specify transport temperature ranges related to the goods item.
FTX | - | C | 9 | - | Free text
This segment is used to provide free form or coded text information related to the entire message.
SG19 | - | C | 9 | - | NAD-DTM
A group of segments to identify different places of collection and/or delivery for the goods item.
NAD | - | M | 1 | - | Name and address
This segment is used to specify the place of delivery for the current goods item.
DTM | - | C | 1 | - | Date/time/period
This DTM segment is used to specify dates and times relating to the delivery party specified in the preceding NAD segment.
SG20 | - | C | 99 | - | MEA-EQN
A group of segments to specify measurements applicable to a goods item.
MEA | - | M | 1 | - | Measurements
This segment is used to specify a measurement for the goods identified in the GID segment. All measurements given in the MEA segments relate to the highest level of packaging (the despatch units) identified in the GID segment.
EQN | - | C | 1 | - | Number of units
This segment is used to specify the number of packages (despatch units) within the goods item to which the measurement applies.
SG21 | - | C | 99 | - | DIM-EQN
A group of segments to specify dimensions applicable to a goods item.
DIM | - | M | 1 | - | Dimensions
This segment is used to indicate the dimensions of the goods item identified in the GID segment. All dimensions given in the DIM segments relate to the highest level packaging (the despatch units) identified in the GID segment.
EQN | - | C | 1 | - | Number of units
This segment is used to specify the number of packages (despatch units) within the goods items to which the dimensions apply.
SG22 | - | C | 9 | - | RFF
A group of segments to identify references to a goods item.
RFF | - | M | 1 | - | Reference
This segment is used to specify references which are applicable to the current goods item only. The references specified here override any specified in segment group 03 in the header.
SG23 | - | C | 9 | - | PCI-GIN
A group of segments to specify marks and numbers of a goods item.
PCI | - | M | 1 | - | Package identification
This segment is used to specify markings and labels on the goods item.
GIN | - | C | 9 | - | Goods identity number
This segment is used to provide identification numbers marked on the packaging of the current goods item.
SG27 | - | C | 999 | - | SGP
A group of segments to specify the distribution of a goods item among the transport equipment.
SGP | - | M | 1 | - | Split goods placement
This segment is used to specify the placement of the goods item in the equipment used for the arriving consignment.
SG30 | - | C | 9 | - | DGS-FTX-SG31-SG32
A group of segments to specify dangerous goods details related to the goods item. One goods item may be in different dangerous goods classes.
DGS | - | M | 1 | - | Dangerous goods
This segment is used to indicate whether the goods item in the arriving consignment contains any dangerous goods.
FTX | - | C | 99 | - | Free text
This segment is used to specify any additional information required for the dangerous goods.
SG31 | - | C | 9 | - | CTA-COM
A group of segments to identify a contact to whom communication regarding the dangerous goods can be directed.
CTA | - | M | 1 | - | Contact information
This segment is used to identify a contact name relating to the dangerous goods identified in the DGS segment.
COM | - | C | 9 | - | Communication contact
This segment identifies the communications number and type of communications for the person or department identified in the preceding CTA segment.
SG32 | - | C | 9 | - | MEA-EQN
A group of segments to identify dangerous goods measurements.
MEA | - | M | 1 | - | Measurements
This segment is used to indicate measurements of the goods item which are dangerous.
EQN | - | C | 1 | - | Number of units
This segment is used to indicate the number of units to which the dangerous goods measurements apply.
SG35 | - | C | 999 | - | EQD-MEA-DIM-SEL-SG37
A group of segments to specify equipment in which goods are transported.
EQD | - | M | 1 | - | Equipment details
This segment is used to indicate the units of equipment which have been used for the transport of the goods items in the arriving consignment.
MEA | - | C | 9 | - | Measurements
This segment is used to specify the gross or tare weight of the equipment identified in the previous EQD segment.
DIM | - | C | 9 | - | Dimensions
This segment is used to indicate the dimensions of the equipment identified in the EQD segment.
SEL | - | C | 99 | - | Seal number
This segment is used to specify a seal number for the equipment identified in the EQD segment.
SG37 | - | C | 9 | - | NAD
A group of segments to identify different equipment pick-up or drop-off places.
NAD | - | M | 1 | - | Name and address
This segment is used to specify the equipment owner, pick up or drop off addresses for the equipment specified in the EQD segment.
Arrival Notice Detail Section
UNT | - | M | 1 | - | MESSAGE TRAILER
This segment is used to end and check the completeness of a message.

(c) Copyright EAN 1997 |