EANCOM PART II |  | 1997-07-01

QUOTES | - | Quote message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 31 |  | Next Segment

SG27 | - | M | 200000 | - | LIN-PIA-IMD-MEA-QTY-ALI-DTM-FTX-SG29-SG31-SG32-SG34-SG39-SG46-SG52-SG54
SG39 | - | C | 10 | - | PAC
PAC | - | M | 1 | - | Package
Function:
To describe the number and type of packages/physical units.
EDIFACT
EAN
*
Description |
7224
Number of packages
C |  | n..8
O
C531
PACKAGING DETAILS
C |
O
| 7075
| Packaging level, coded |
C |  | an..3
N
| 7233
| Packaging related information, coded |
C |  | an..3
O
50 = Package barcoded EAN-13 or EAN-8
51 = Package barcoded ITF-14 or ITF-6
52 = Package barcoded UCC or EAN-128
| 7073
| Packaging terms and conditions, coded |
C |  | an..3
O
1 = Packaging cost paid by supplier
2 = Packaging cost paid by recipient
C202
PACKAGE TYPE
C |
R
| 7065
| Type of packages identification |
C |  | an..17
A
AE = Aerosol
CX = Can, cylindrical
CS = Case
| 1131
| Code list qualifier |
C |  | an..3
O
| 3055
| Code list responsible agency, coded |
C |  | an..3
O
| 7064
| Type of packages |
C |  | an..35
O
C402
PACKAGE TYPE IDENTIFICATION
C |
N
| 7077
| Item description type, coded |
M |  | an..3
| 7064
| Type of packages |
M |  | an..35
| 7143
| Item number type, coded |
C |  | an..3
| 7064
| Type of packages |
C |  | an..35
| 7143
| Item number type, coded |
C |  | an..3
C532
RETURNABLE PACKAGE DETAILS
C |
D
| 8395
| Returnable package freight payment responsibility, coded |
C |  | an..3
O
1 = Paid by customer
3 = Paid by supplier
| 8393
| Returnable package load contents, coded |
C |  | an..3
N
Segment Notes:
This segment is used to identify the type of packaging being used for the current line item. Example : PAC+1++CS' Dependency Notes : Composite C532 is only used where the packaging being described is returnable. This composite identifies who is responsible for the payment of its return.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |