EANCOM PART II |  | 1997-07-01

IFTMAN | - | Arrival notice message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 38 |  | Next Segment

SG35 | - | C | 999 | - | EQD-MEA-DIM-SEL-SG37
EQD | - | M | 1 | - | Equipment details
Function:
To identify a unit of equipment.
EDIFACT
EAN
*
Description |
8053
Equipment qualifier
M |  | an..3
M
CN = Container
PA = Pallet
UL = ULD (Unit load device)
BPN = Box pallet non exchangeable
EFP = Exchangeable EUR flat pallet
C237
EQUIPMENT IDENTIFICATION
C |
R
| 8260
| Equipment identification number |
C |  | an..17
O
| 1131
| Code list qualifier |
C |  | an..3
O
| 3055
| Code list responsible agency, coded |
C |  | an..3
O
9 = EAN (International Article Numbering association)
| 3207
| Country, coded |
C |  | an..3
O
C224
EQUIPMENT SIZE AND TYPE
C |
O
| 8155
| Equipment size and type identification |
C |  | an..10
O
6 = Pressurized tank
21 = Container IC 20 ft.
| 1131
| Code list qualifier |
C |  | an..3
O
| 3055
| Code list responsible agency, coded |
C |  | an..3
O
| 8154
| Equipment size and type |
C |  | an..35
O
8077
Equipment supplier, coded
C |  | an..3
O
1 = Shipper supplied
2 = Carrier supplied
8249
Equipment status, coded
C |  | an..3
O
8169
Full/empty indicator, coded
C |  | an..3
O
4 = Empty
5 = Full
Segment Notes:
This segment is used to indicate the units of equipment which have been used for the transport of the goods items in the arriving consignment. Example : EQD+UL+45223'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |