EANCOM PART II |  | 1997-07-01

RECADV | - | Receiving advice message | VERSION | 003

5. Segments Layout |

Previous Segment |  | Segment number: | 16 |  | Next Segment

SG16 | - | C | 9999 | - | CPS-SG17-SG22
SG22 | - | C | 9999 | - | LIN-PIA-QTY-QVR-DTM-SG28-SG29
LIN | - | M | 1 | - | Line item
Function:
To identify a line item and configuration.
EDIFACT
EAN
*
Description |
1082
Line item number
C |  | n..6
R
Application generated number of the line item within the Receiving Advice.
1229
Action request/notification, coded
C |  | an..3
N
C212
ITEM NUMBER IDENTIFICATION
C |
D
| 7140
| Item number |
C |  | an..35
R
Format n..14 EAN-8, UPC-A, EAN-13, or DUN-14 - this is the number of the article which has been received. |
| 7143
| Item number type, coded |
C |  | an..3
R
*
EN = International Article Numbering Association (EAN)
UP = UPC (Universal product code)
| 1131
| Code list qualifier |
C |  | an..3
N
| 3055
| Code list responsible agency, coded |
C |  | an..3
O
C829
SUB-LINE INFORMATION
C |
D
| 5495
| Sub-line indicator, coded |
C |  | an..3
R
*
1 = Sub-line information
| 1082
| Line item number |
C |  | n..6
R
1222
Configuration level
C |  | n..2
N
7083
Configuration, coded
C |  | an..3
D
A = Added to the configuration
D = Deleted from the configuration
I = Included in the configuration
Segment Notes:
This segment is used to identify the product delivered. If a product has been delivered but not accepted it must be identified using a separate line item. In these cases the received and accepted quantities are zero. Such products might include unknown or not ordered products, excess deliveries, damaged goods, unacceptable product variants or batch numbers, different pack size, etc,. Reasons for the action is detailed in the QTY-QVA-DTM segments. Example : LIN+1++5412345123453:EN' Dependency Notes : DE C212: This composite will only be used for the identification of EAN/UPC codes. If another coding structure is required, e.g. HIBC, this composite will not be used and the code will be detailed in the PIA segment. DE's C829 and 7083: These data elements are only used when sub-lines are required. FOR A COMPLETE DESCRIPTION ON THE USAGE OF SUB-LINES PLEASE REFER TO PART I, SECTION 4.11 .

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |