EANCOM PART II |  | 1997-07-01

DESADV | - | Despatch advice message | VERSION | 005

5. Segments Layout |

Previous Segment |  | Segment number: | 46 |  | Next Segment

SG10 | - | C | 9999 | - | CPS-SG11-SG15
SG15 | - | C | 9999 | - | LIN-PIA-IMD-MEA-QTY-DLM-DTM-FTX-SG16-SG18-SG20-SG23
SG23 | - | C | 10 | - | QVR-DTM
QVR | - | M | 1 | - | Quantity variances
Function:
To specify item details relating to quantity variances. Note: This segment replaces segment QVA (which has been deleted in this directory).
EDIFACT
EAN
*
Description |
C279
QUANTITY DIFFERENCE INFORMATION
C |
R
| 6064
| Quantity difference |
M |  | n..15
M
Specify the actual variance amount here. |
| 6063
| Quantity qualifier |
C |  | an..3
R
*
21 = Ordered quantity
66 = Committed quantity
4221
Discrepancy, coded
C |  | an..3
O
BP = Shipment partial - back order to follow
CP = Shipment partial - considered complete, no backorder
C960
REASON FOR CHANGE
C |
O
| 4295
| Change reason, coded |
C |  | an..3
O
| 1131
| Code list qualifier |
C |  | an..3
O
| 3055
| Code list responsible agency, coded |
C |  | an..3
O
9 = EAN (International Article Numbering association)
| 4294
| Change reason |
C |  | an..35
O
Segment Notes:
This segment is used to specify any variances between what was ordered and what is ready for or has been despatched. The quantity identified in DE 6064 must always refer to the difference between the despatched quantity identified in DE 6060 of QTY at LIN level and the ordered quantity. For negative values (e.g. damaged goods not accepted) the variance must be expressed as negative. Example : QVR+-50:21' The QTY at line level identified the fact that 450 units were ordered and that 400 were being despatched, so therefore the quantity variance is 50 units.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |