EANCOM PART II |  | 1997-07-01

MSCONS | - | Metered services consumption report | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 30 |  | Next Segment

CNT | - | C | 99 | - | Control total
Function:
To provide control total.
EDIFACT
EAN
*
Description |
C270
CONTROL
M |
M
| 6069
| Control qualifier |
M |  | an..3
M
*
32 = Number of meters (EAN Code)
31E = Number of premises (EAN Code)
| 6066
| Control value |
M |  | n..18
M
| 6411
| Measure unit qualifier |
C |  | an..3
O
Segment Notes:
This is used to provide message control information for checking on the message receivers in-house system. DE 6066: When using code '31E' this figure is calculated by counting the ttotal number of NAD segments in gegment group 5. When using code '32E' this figure is calculated by counting the ttotal number of LOC segments in gegment group 6. Example : CNT+32:45'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |