EANCOM PART II |  | 1997-07-01

INVRPT | - | Inventory report message | VERSION | 004

5. Segments Layout |

Previous Segment |  | Segment number: | 24 |  | Next Segment

SG9 | - | C | 9999 | - | LIN-PIA-IMD-SG11
SG11 | - | C | 9999 | - | QTY-INV-GIN-LOC-DTM-STS-SG13-SG14-SG15
SG15 | - | C | 9999 | - | CPS-SG16
CPS | - | M | 1 | - | Consignment packing sequence
Function:
To identify the sequence in which physical packing is presented in the consignment, and optionally to identify the hierarchical relationship between packing layers.
EDIFACT
EAN
*
Description |
7164
Hierarchical id. number
M |  | an..12
M
Sequential numbering recommended.
7166
Hierarchical parent id.
C |  | an..12
O
7075
Packaging level, coded
C |  | an..3
N
Segment Notes:
This segment is used to provide a detailed description of the packaging of the goods held in stock. DE 7164: When not identifying different packaging hierarchical levels within the Inventory Report, it is recommended to use a default value of 1. Example : CPS+1'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |