EANCOM PART II |  | 1997-07-01

QALITY | - | Quality data message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 15 |  | Next Segment

SG5 | - | C | 200 | - | LIN-PIA-IMD-MEA-DTM-QTY-FTX-SG6-SG7-SG12
MEA | - | C | 10 | - | Measurements
Function:
To specify physical measurements, including dimension tolerances, weights and counts.
EDIFACT
EAN
*
Description |
6311
Measurement application qualifier
M |  | an..3
M
PD = Physical dimensions (product ordered)
SV = Specification value
C502
MEASUREMENT DETAILS
C |
A
| 6313
| Measurement dimension, coded |
C |  | an..3
A
AAU = Operative temperature
DI = Diameter
LN = Length dimension
| 6321
| Measurement significance, coded |
C |  | an..3
O
3 = Approximately
4 = Equal to
| 6155
| Measurement attribute, coded |
C |  | an..3
O
| 6154
| Measurement attribute |
C |  | an..70
O
C174
VALUE/RANGE
C |
R
| 6411
| Measure unit qualifier |
M |  | an..3
M
CEL = Degree celsius
FAH = Degree Fahrenheit
MMT = Millimetre
VLT = Volt
| 6314
| Measurement value |
C |  | n..18
O
| 6162
| Range minimum |
C |  | n..18
O
| 6152
| Range maximum |
C |  | n..18
O
| 6432
| Significant digits |
C |  | n..2
N
7383
Surface/layer indicator, coded
C |  | an..3
N
Segment Notes:
This segment is used to specify measurements relative to the item which has been tested, e.g. the weight of the item tested, range of temperatures which a meter should cater for, etc. Example : MEA+SV+AAU+CEL::20:150' The current item has a specification value in the range of 20 to 150 degrees celsius.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |