EANCOM PART II |  | 1997-07-01

CONTRL | - | Control message | VERSION | 002

4. Segments Description |

Syntax And Service Report Heading Section
UNH | - | M | 1 | - | MESSAGE HEADER
This segment is used to head, identify and specify a message.
UCI | - | M | 1 | - | INTERCHANGE RESPONSE
This segment is used to identify the interchange being responded to.
SG1 | - | C | 999999 | - | UCM-SG2
A group of segments sent in response to a message in the subject interchange identified in the UCI segment. This segment group is only used if the subject interchange does not contain functional groups.
Syntax And Service Report Detail Section
UCM | - | M | 1 | - | MESSAGE RESPONSE
This segment is used to identify specific messages within the interchange identified in the previous UCI segment.
SG2 | - | C | 999 | - | UCS-UCD
A group of segments sent in response to a segment containing one or more errors, and which was part of the message identified by the UCM segment in segment group 1.
UCS | - | M | 1 | - | SEGMENT ERROR INDICATION
This segment is used to identify the position of a segment within a message. This segment is only used to identify segments within the message identified in the UCM segment which have errors.
Syntax And Service Report Summary Section
UCD | - | C | 99 | - | DATA ELEMENT ERROR INDICATOR
This segment is used to identify the position of a component or composite data element within a segment. This segment is only used to identify component or composite data elements within the segment identified in the UCS segment which have errors.
UNT | - | M | 1 | - | MESSAGE TRAILER
This segment is a mandatory UN/EDIFACT segment. It must always be the last segment in the message.

(c) Copyright EAN 1997 |