EANCOM PART II |  | 1997-07-01

IFCSUM | - | Forwarding and consolidation summary message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 55 |  | Next Segment

SG15 | - | C | 9999 | - | CNI-DTM-CNT-TSR-MOA-FTX-SG21-SG22-SG30-SG37-SG56
SG37 | - | C | 999 | - | GID-HAN-TMP-RNG-MOA-PIA-FTX-SG38-SG39-SG40-SG41-SG42-SG43-SG48-SG51
SG42 | - | C | 9 | - | PCI-GIN
GIN | - | C | 9 | - | Goods identity number
Function:
To give specific identification numbers, either as single numbers or ranges.
EDIFACT
EAN
*
Description |
7405
Identity number qualifier
M |  | an..3
M
*
BJ = Serial shipping container code
C208
IDENTITY NUMBER RANGE
M |
M
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
N
C208
IDENTITY NUMBER RANGE
C |
O
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
N
C208
IDENTITY NUMBER RANGE
C |
O
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
N
C208
IDENTITY NUMBER RANGE
C |
O
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
N
C208
IDENTITY NUMBER RANGE
C |
O
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
N
Segment Notes:
This segment is used to provide the Serial Shipping Container Code which has been marked on the packaging of the current goods item. In EANCOM it is recommended to use the Serial Shipping Container Code (SSCC) for the unique identification of individual transport packages. Example : GIN+BJ+354123450000000014'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |