EANCOM PART II |  | 1997-07-01

CONTRL | - | Control message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 2 |  | Next Segment

UCI | - | M | 1 | - | INTERCHANGE RESPONSE
Function:
To identify the subject interchange, to indicate acknowledgement or rejection (action taken) of the UNA, UNB and UNZ segments, and to identify any error related to these segments. Depending on the action code it may also indicate the action taken on the functional groups and messages within that interchange.
EDIFACT
EAN
*
Description |
0020
Interchange control reference
M |  | an..14
M
S002
INTERCHANGE SENDER
M |
M
| 0004
| Sender identification |
M |  | an..35
M
| 0007
| Partner identification code qualifier |
C |  | an..4
O
*
14 = EAN International
| 0008
| Address for reverse routing |
C |  | an..14
O
S003
INTERCHANGE RECIPIENT
M |
M
| 0010
| Recipient identification |
M |  | an..35
M
| 0007
| Partner identification code qualifier |
C |  | an..4
O
*
14 = EAN International
| 0014
| Routing address |
C |  | an..14
O
0083
Action, coded
M |  | an..3
M
4 = This level and all lower levels rejected
6 = UNB/UNZ rejected
7 = This level acknowledged, next lower level acknowledged if not explicitly rejected
8 = Interchange received
0085
Syntax error, coded
C |  | an..3
D
*
2 = Syntax level or version not supported
7 = Interchange recipient not actual recipient
12 = Invalid value
13 = Missing
14 = Value not supported in this position
15 = Not supported in this position
16 = Too many constituents
17 = No agreement
18 = Unspecified error
19 = Invalid decimal notation
20 = Character invalid as service character
21 = Invalid character(s)
22 = Invalid service character(s)
23 = Unknown interchange sender
24 = Too old
25 = Test indicator not supported
26 = Duplicate detected
27 = Security function not supported
28 = References do not match
29 = Control count does not match number of instances received
30 = Functional groups and messages mixed
32 = Lower level empty
33 = Invalid occurrence outside message or functional group
37 = Invalid type of character(s)
39 = Data element too long
40 = Data element too short
41 = Permanent communication network error
42 = Temporary communication network error
43 = Unknown interchange recipient
0013
Segment tag, coded
C |  | a3
D
S011
DATA ELEMENT POSITION
C |
D
| 0098
| Erroneous data element position in segment |
M |  | n..3
M
| 0104
| Erroneous component data element position |
C |  | n..3
O
Segment Notes:
This segment is used to identify the interchange being responded to. The segment may also be used to indicate acknowledgement or rejection of the UNA, UNB and UNZ segments and any errors present in these segments. DE's 0020, S002 and S003: To identify the interchange being responded to these data elements must contain the same values as were specified in the UNB segment of the original interchange. DE's 0083 and 0085: These data elements are used to indicate the status of the interchange and in cases where errors are present to identify the error. DE's 0013, S011: If there are errors in the UNA, UNB or UNZ segments the segment in question and the position of the error in the segment may be identified in these data elements. DE 0098: The numerical count position of the simple or composite data element in error. The segment tag and each simple and composite data element position number within the segment. DE 0104: The numerical count position of the component data element in error. Each component data element position defined in the composite data element description shall cause the count to be incremented. Example : UCI+10001+5412345000013:14+5412345000020:14+8' Interchange number 10001 from the party identified by the EAN location number 5412345000013 to the party identified by the EAN location number 5412345000020 has been received. Dependency Notes : Data elements 0085, 0013 and S011 are only used when errors are being reported.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |