EANCOM PART II |  | 1997-07-01
HANMOV | - Cargo/Goods Handling and Movement Message | VERSION 002

## 6. Examples

### Example 5

The following is an example of a Cargo/goods handling and movement message sent from a supplier identified by the EAN location number 5098765222220 to his logistic service provider identified by the EAN location number 5071615222229. The message is dated the 4th of January 1997 and has the message reference WH0655.

The message requests the logistic services provider to pick the products and quantities detailed in sequence, to pack them on the pallets specified, and to label the pallets according to the details provided.

EAN Article Number | Quantity | Pallet type | Units per layer | SSCC
4000862141404 * | 20 | 1/4 Euro | 20 | 354123450000000014
5412345111184 * | 12 | 1/4 Euro | 12 | 354123450000000014
4000862141411 | 10 | 1/8 Euro | 10 | 354107380000001051

Note :
The product identified by the EAN article number 5412345111184 is to be picked and packed on the pallet first, with the product identified by the EAN article number 4000862141404 packed on the same pallet on top of the first product picked.

UNH+1+HANMOV:D:96A:EN:EAN002' | Message header
BGM+90E::9+WH0655+9' | Cargo/goods handling and movement number WH6222
DTM+137:19970104:102' | Message date 4th of January 1997
HAN+PKS::9' | Message requests picking in sequence service
HAN+PAC::9' | and packing services
HAN+LAB::9' | and labelling services
NAD+SU+5098765222220::9' | Supplier is identified by the EAN location number 5098765222220
NAD+LSP+5071615222229::9' | Logistic service provider is identified by the EAN location number 5071615222229
LIN+1++5412345111184:EN' | First product to be picked is identified by the EAN article number 5412345111184
QTY+1:12' | 12 units subject to the instruction
PAC+1+::3E+203::9' | Product is to be packed in one 1/4 Euro pallet
MEA+PD+ULY+PCE:12' | With 10 pieces per layer
QTY+52:12' | Quantity per pack is 12
PCI+30' | The pallet is to be marked with a Serial Shipping Container Code
GIN+BJ+354123450000000014' | Serial Shipping Container Code 354123450000000014 is to be marked
LIN+2++4000862141404:EN' | Second product to be picked is identified by the EAN article number 4000862141404
QTY+1:20' | 20 units subject to the instruction
PAC+1+::3E+203::9' | Product is to be packed in one 1/4 Euro pallet
MEA+PD+ULY+PCE:20' | With 20 pieces per layer
QTY+52:20' | Quantity per pack is 20
PCI+30' | The pallet is to be marked with a Serial Shipping Container Code
GIN+BJ+354123450000000014' | Serial Shipping Container Code 354123450000000014 is to be marked
LIN+3++4000862141411:EN' | Second product to be picked is identified by the EAN article number 4000862141411
QTY+1:10' | 10 units subject to the instruction
PAC+1+::3E+204::9' | Product is to be packed in one 1/8 Euro pallet
QTY+52:10' | Quantity per pack is 10
PCI+30' | The pallet is to be marked with a Serial Shipping Container Code
GIN+BJ+354107380000001051' | Serial Shipping Container Code 354107380000001051 is to be marked
UNT+29+1' | Message trailer - 29 segments in the message

(c) Copyright EAN 1997