EANCOM PART II |  | 1997-07-01

IFTMAN | - | Arrival notice message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 39 |  | Next Segment

SG35 | - | C | 999 | - | EQD-MEA-DIM-SEL-SG37
MEA | - | C | 9 | - | Measurements
Function:
To specify physical measurements, including dimension tolerances, weights and counts.
EDIFACT
EAN
*
Description |
6311
Measurement application qualifier
M |  | an..3
M
*
AAE = Measurement
C502
MEASUREMENT DETAILS
C |
A
| 6313
| Measurement dimension, coded |
C |  | an..3
A
AAD = Total gross weight
T = Tare weight
| 6321
| Measurement significance, coded |
C |  | an..3
N
| 6155
| Measurement attribute, coded |
C |  | an..3
O
| 6154
| Measurement attribute |
C |  | an..70
N
C174
VALUE/RANGE
C |
R
| 6411
| Measure unit qualifier |
M |  | an..3
M
KGM = Kilogram
TNE = Metric ton (1000kg)
| 6314
| Measurement value |
C |  | n..18
O
| 6162
| Range minimum |
C |  | n..18
O
| 6152
| Range maximum |
C |  | n..18
O
| 6432
| Significant digits |
C |  | n..2
N
7383
Surface/layer indicator, coded
C |  | an..3
N
Segment Notes:
This segment is used to specify the gross or tare weight of the equipment identified in the previous EQD segment. Example : MEA+AAE+AAD+KGM:622'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |