EANCOM PART II |  | 1997-07-01

QUOTES | - | Quote message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 36 |  | Next Segment

SG27 | - | M | 200000 | - | LIN-PIA-IMD-MEA-QTY-ALI-DTM-FTX-SG29-SG31-SG32-SG34-SG39-SG46-SG52-SG54
SG46 | - | C | 99 | - | ALC-SG47-SG48-SG49-SG50-SG51
SG48 | - | C | 10 | - | PCD-RNG
RNG | - | C | 1 | - | Range details
Function:
To identify a range.
EDIFACT
EAN
*
Description |
6167
Range type qualifier
M |  | an..3
M
1 = Allowance range
2 = Charge range
C280
RANGE
C |
R
| 6411
| Measure unit qualifier |
M |  | an..3
M
KGM = Kilogram
LTR = Litre (1 dm3)
PCE = Piece
| 6162
| Range minimum |
C |  | n..18
A
| 6152
| Range maximum |
C |  | n..18
O
Segment Notes:
This segment is used to indicate ranges which must be satisfied before which the percentage allowance or charge becomes effective. Example : RNG+1+PCE:50'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |