EANCOM PART II |  | 1997-07-01

DESADV | - | Despatch advice message | VERSION | 005

5. Segments Layout |

Previous Segment |  | Segment number: | 17 |  | Next Segment

SG10 | - | C | 9999 | - | CPS-SG11-SG15
CPS | - | M | 1 | - | Consignment packing sequence
Function:
To identify the sequence in which physical packing is presented in the consignment, and optionally to identify the hierarchical relationship between packing layers.
EDIFACT
EAN
*
Description |
7164
Hierarchical id. number
M |  | an..12
M
Sequential numbering recommended.
7166
Hierarchical parent id.
C |  | an..12
A
7075
Packaging level, coded
C |  | an..3
N
Segment Notes:
This segment is used to identify the sequence in which packing of the consignment occurs. Please refer to the Structure of the Despatch Advice Message section in the introduction for details on the use of the CPS segment (see pages 2 to 5). Example : CPS+1'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |