EANCOM PART II |  | 1997-07-01

HANMOV | - | Cargo/goods handling and movement message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 21 |  | Next Segment

SG7 | - | C | 99 | - | LIN-PIA-IMD-HAN-SG8-QTY-DTM-FTX-SG10-SG11
SG11 | - | C | 99 | - | PAC-MEA-QTY-SG12
MEA | - | C | 9 | - | Measurements
Function:
To specify physical measurements, including dimension tolerances, weights and counts.
EDIFACT
EAN
*
Description |
6311
Measurement application qualifier
M |  | an..3
M
PD = Physical dimensions (product ordered)
C502
MEASUREMENT DETAILS
C |
A
| 6313
| Measurement dimension, coded |
C |  | an..3
A
AEA = Loading height
AEB = Stacking height
HT = Height dimension
LAY = Number of layers (EAN Code)
LN = Length dimension
ULY = Number of units per layer (EAN Code)
WD = Width dimension
| 6321
| Measurement significance, coded |
C |  | an..3
O
3 = Approximately
4 = Equal to
| 6155
| Measurement attribute, coded |
C |  | an..3
N
| 6154
| Measurement attribute |
C |  | an..70
N
C174
VALUE/RANGE
C |
R
| 6411
| Measure unit qualifier |
M |  | an..3
M
CMT = Centimetre
MTQ = Cubic metre
PCE = Piece
| 6314
| Measurement value |
C |  | n..18
O
| 6162
| Range minimum |
C |  | n..18
O
| 6152
| Range maximum |
C |  | n..18
O
| 6432
| Significant digits |
C |  | n..2
O
7383
Surface/layer indicator, coded
C |  | an..3
N
Segment Notes:
This segment is used to provide measurements relevant to the packaging described in the PAC segment. Example : MEA+PD+ULY+PCE:12'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |