EANCOM PART I |  |

Segment Layout | - UNE segment

UNE | - | C | 1 | - | FUNCTIONAL GROUP TRAILER
Function:
To end and check the completeness of a functional group.
EDIFACT
EAN
*
Description |
0060
Number of messages
M |  | n..6
M
Number of messages in the group. |
0048
Functional group reference number
M |  | an..14
M
Identical to DE 0048 in UNG segment. |
Segment Notes:
Within EANCOM the use of the UNG..UNE segments is not recommended as the grouping of same message types is not considered to add significant value to simply including multiple same message types within one interchange, i.e. between UNB..UNZ.

(c) Copyright EAN 2002 |